








ARYAMAN MISHRA

19BCE1027

1) 16-bit division of two numbers from the memory location 3000H to 3003H and write the result into 4000H to 4003H locations.



2) Sum of all elements stored in a data segment (for six eight-bit data's)



3) Average of six eight-bit data's stored in the data segment

